STANDARD SPECIFICATION 
PURITY OF MORPHOLINE: ＞99.0% MIN (BY GAS CHROMATOGRAPHY)
COLOUR: ≤10  #   APHA
SPECIFIC GRAVITY (20OC): 0.999—1.002

BOILING RANGE: 126-129OC
WATER CONTENT (MOISTURE)： ≤0.3%
PH:>11

Appearance:Clear and substantially free of suspended matter

Flash point:31-35  ˚C

